# GEX 12V-77: Changing the Sanding Pad (see figures E–F)

- Before carrying out any work on the power tool (e.g. maintenance, tool change etc.), remove the battery from the power tool. There is risk of injury from unintentionally pressing the on/off switch.

Note: Replace damaged sanding pads (2) immediately.

Pull off the sanding sheet.

Disassembly: Hold the spanner flat (11) on the power tool with the open-ended spanner (10) and turn the sanding pad (2) counterclockwise to remove it (see figure E).

Clean all the parts to be fitted.

Assembly: Hold the spanner flat (11) on the power tool in place with an open-ended spanner (10). Tighten the new sanding pad (2) clockwise (see figure F).

Note: When attaching the sanding pad, make sure that the teeth of the catch mate with the recesses in the sanding pad.