# Battery charge indicator

The 5 LEDs of the LED display will indicate the state of charge of the battery. The LED indicator lights up for 5 seconds after start-up.

LED | Capacity
--- | ---
5 × continuous green light | 80–100 %
4 × continuous green light | 60–80 %
3 × continuous green light | 40–60 %
2 × continuous green light | 20–40 %
1 × continuous yellow light | 1–20 %
1 × continuous red light | 0–1 %

## Temperature-dependent overload protection

In normal conditions of use, the power tool cannot be overloaded. If the power tool is overloaded or not kept within the permitted battery temperature range, the speed is reduced or the power tool switches off. At reduced speed, the power tool will run again at full speed once the permitted battery temperature is reached or the load is reduced. If it automatically shuts down, switch the power tool off, allow the battery to cool down, then switch the power tool back on.