# Changing the Sanding Sheet (see figures A–B)

To remove the sanding sheet (9), lift it from the side and pull it from the sanding pad (2).

Remove dirt and dust from the sanding pad (2), e.g. with a paintbrush, before attaching a new sanding sheet.

The surface of the sanding pad (2) is fitted with a hook-and-loop fastening, allowing sanding sheets with a hook-and-loop backing to be secured quickly and easily.

A sanding pad with a smooth surface can also be attached in order to use adhesive sanding paper.

Press the sanding sheet (9) firmly onto the underside of the sanding pad (2).