# Practical advice

After working at a low speed for an extended period, you should operate the power tool at the maximum speed for approximately three minutes without load to cool it down.

Belt clip (see figures K–L)

You can use the belt clip (11) to hang the adapter on a belt, for example. You then have both hands free and the adapter is always at hand.

- When fitting it, ensure that the snap-in pin (15) on the belt clip engages in the recess of the adapter housing.

- To remove the belt clip, lift the snap-in pin (15) using a sharp object and pull off the belt clip.