# Technical Data

Hammer adapter with auxiliary handle |  | GFA 12-H | GFA 12-H | GFA 12-H
--- | --- | --- | --- | ---
Article number |  | ‎1 600 A01 L1N | ‎1 600 A01 L1N | ‎1 600 A01 L1N
Cordless screwdriver |  | GSR 12V-15 FC | GSR 12V-32 FC | GSR 12V-35 FC
Article number |  | ‎3 601 JF6 0..  ‎ | 3 601 JN7 1..  ‎ | ‎3 601 JH3 0..
Rated speedA) | min-1 | 0–1300 | 0–1800 | 0–1750
Impact rateA) | min-1 | 0–2600 | 0–3500 | 0–3700
Rated voltage | V= | 12 | 12 | 12
Tool holder |  | SDS plus | SDS plus | SDS plus
Max. drilling diameter |  |  |  |
Concrete | mm | 10 | 10 | 10
Masonry | mm | 16 | 16 | 16
WeightB) | kg | 1.4 | 1.3 | 1.4
Recommended ambient temperature during charging | °C | 0 to +35 | 0 to +35 | 0 to +35
Permitted ambient temperature during operationC) and during storage | °C | –20 to +50 | –20 to +50 | –20 to +50

A)

  Measured at 20–25 °C with rechargeable battery GBA 12V 6.0Ah

B)

  With auxiliary handle, without rechargeable battery (you can find the battery weight at www.bosch-professional.com.)

C)

  Limited performance at temperatures < 0 °C

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.