# Technical Data

Cordless Drill/Driver |  | GSR 12V-32 FC | GFA 12-X | GFA 12-M | GFA 12-E | GFA 12-W | GFA 12-B
--- | --- | --- | --- | --- | --- | --- | ---
Article number |  | ‎3 601 JN7 1..‎ | – | – | – | – | –
Rated voltage | V= | 12 | – | – | – | – | –
No-load speedA)
First gear | min-1 | 0–475 | – | – | – | – | –
Second gear | min-1 | 0–1800 | – | – | – | – | –
Max. torque, hard/soft screwdriving application according to ISO 5393A) | Nm | 32/21 | – | – | – | – | –
Max. drilling diameter (1st/2nd gear)
Steel | mm | 10 | – | – | – | – | –
Wood | mm | 35 | – | – | – | – | –
Max. screw diameter | mm | 8 | – | – | – | – | –
Tool holder | mm | 6.35 (¼") | 6.35 (¼") | 0.8–10 | 6.35 (¼") | 6.35 (¼") | 0.8–10
Weight | kg | 0.6B) | 0.10 | 0.20 | 0.30 | 0.30 | 0.20
Recommended ambient temperature during charging | °C | 0 to +35 | – | – | – | – | –
Permitted ambient temperature during operation and during storage | °C | –20 to +50 | – | – | – | – | –
Recommended rechargeable batteries |  | GBA 12V... | – | – | – | – | –
Recommended battery chargers |  | GAL 12... GAX 18... | – | – | – | – | –

A)

  Measured at 20−25 °C with battery GBA 12V 6.0Ah and attachment GFA 12-M

B)

  Weight without rechargeable battery
  (Weight of rechargeable battery can be found on http://www.bosch-professional.com)

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.