# Changing the tool

##

Insert the application tool all the way into the tool holder (1).

##

Remove the application tool.

Insert the attachment into the tool holder (1). Turn the locking ring (15) until it audibly clicks into place.

##

GFA 12-W (see figure A)

Insert the application tool all the way into the tool holder (1).

GFA 12-E, GFA 12-X (see figure C)

Push back the locking sleeve , guide the application tool into the tool holder (1) as far as it will go and release the locking sleeve to lock the application tool.

GFA 12-M/GFA 12-B (see figure D)

Open the (metal) drill chuck attachment (11) by turning it in the direction of rotation ➊ until the application tool can be inserted. Insert the application tool.

Firmly tighten the sleeve of the (metal) drill chuck attachment (11) by turning it by hand in the direction of rotation ➋. This will automatically lock the (metal) drill chuck.

To release the locking mechanism and remove the tool, turn the sleeve of the (metal) drill chuck attachment (11) in the direction of rotation ➊.

##

Pull the attachment forwards. Turn the attachment. The attachment clicks into place in 16 positions around a 360° axis. Choose a position that is suitable for the work being carried out.

Let go of the attachment again to lock it.

##

Remove the application tool.

Unlock the attachment in direction and pull it off the tool holder (1).

##

The right angle attachment (13) can be combined with any of the other attachments.

To do this, insert the right angle attachment (13) into the tool holder (1). Turn the locking ring (15) until it audibly clicks into place. Then attach one of the other attachments to the right angle attachment (13).