# Technical data

Wet/dry dust extractor | GAS12‑25LS
--- | ---
Article number |  | ‎3 601 JS3 1..‎‎‎‎
Rated power input | W | 1200
Frequency | Hz | 50–60
Container volume (gross) | l | 25
Net volume (liquid) | l | 18
Net volume (dry) | l | 20
Volume of fleece filter bag | l | 10
Vacuum pressure
Dust extractorA) | hPa | 200
Turbine | hPa | 210
Flow rate
Dust extractorA) | m³/h l/s | 126 35
Turbine | m³/h l/s | 234 65
Dust class |  | L
WeightB) | kg | 9.4
Protection class |  | /I
Protection rating |  | IPX4

A)

  Measured using a vacuum hose which is 3.1 m long with an inner diameter of 32 mm

B)

  Without mains connection cable

The specifications apply to a rated voltage [U] of 230 V. These specifications may vary at different voltages and in country-specific models.

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.

## Plug socket on the dust extractor

Permitted connected load of the connected power tool
‎3 601 JS3 … | Rated voltage | Maximum power | Minimum power
--- | --- | --- | ---
‎… 100/… 1W0 | 230 V | 2100 W | 100 W
‎… 130‎ | 230 V | 1000 W | 100 W
‎… 170‎/… 1L0 | 220−240 V | 1660 W | 100 W
… 180/… 1B0/… 1E0/… 1N0‎ | 220 V | 2100 W | 100 W
‎… 1H0‎ | 220 V | 1000 W | 100 W
‎… 1K0‎ | 220−240 V | 2100 W | 100 W

Permitted connected load of the connected power tool.
These values can differ for other country-specific models. Please take note of the information on the socket of the dust extractor.