# Starting Operation

- Check the mains voltage! The voltage of the power source must correspond with the information on the type plate of the dust extractor.

- Make sure you inform yourself about the applicable regulations/laws on how to handle harmful types of dust in your country.

The dust extractor may be used for vacuuming and extracting the following materials:

- Dusts with an exposure limit of > 1 mg/m3

- Products that are only sold in AUS and NZ: Use a residual current device (RCD) with a nominal residual current of 30 mA or less.

The dust extractor must categorically not be used in potentially explosive areas.

To ensure optimum suction power, you must always fully unwind the vacuum hose (23) from the top part of the dust extractor (12).

## Switching On and Off

To switch on the dust extractor, push the mode selector switch (4) to position 1.

To switch on the automatic start/stop feature, push the mode selector switch (4) to position 1+. The dust extractor can be started automatically if it is connected to a power tool via the plug socket (6).

To switch off the dust extractor, push the mode selector switch (4) to position 0.