# Fitting the vacuuming accessories (see figure G)

The vacuum hose (23) is equipped with a clip system which can be used to connect vacuuming accessories (dust extraction adapter (27), curved nozzle (28)).

## Fitting the nozzles and tubes

- Push the curved nozzle (28) onto the vacuum hose (23) until you hear both snap fasteners (26) on the vacuum hose engage.
- Then attach the required extraction accessory (floor nozzle, crevice nozzle, suction tube, etc.) firmly to the curved nozzle (28).
- To remove the accessory, press the snap fasteners (26) inwards and pull apart the components.

## Fitting the dust extraction adapter

- Push the dust extraction adapter (27) onto the vacuum hose (23) until you hear both snap fasteners (26) on the vacuum hose engage.
- To remove the adapter, press the snap fasteners (26) inwards and pull apart the components.