# Assembly

- Pull the plug out of the socket before cleaning or performing maintenance on the dust extractor, making tool adjustments, changing accessories or putting away the dust extractor. This safety measure prevents the dust extractor from being started accidentally.

Inserting/Removing the Fleece Filter Bag
Fitting the Bracket for Extractor Accessories
Fitting the Hose
Fitting the Extraction Accessories
Removing/Inserting the Insert for the Floor Nozzle
Attaching the L-Boxx