# Noise/Vibration Information

Noise emission values determined according to EN 60335‑2‑69.

Typically the A-weighted sound pressure level of the dust extractor is 75 dB(A). Uncertainty K = 2 dB. The noise level when working can exceed the volume stated. Wear hearing protection!

Vibration values ah (continuous vibrations), pF (repeated shock vibrations) and uncertainty K determined according to EN 60335‑2‑69:

ah = 0.2 m/s2 (K = 1.5 m/s2), pF = 4 m/s2 (K = 1 m/s2)