# Fitting the Bracket for Extractor Accessories (see figures C−D)

Push the holder (10) for the extraction accessory into the adapter provided for it on the upper part of the extractor until it engages.
To remove the holder (10), pull the locking mechanism (22) on the underside of the holder and push the holder up out of the adapter.

The holder (10) can also be secured to the wall using 2 screws.