# Rotating the machine head (see figure E)

- Before carrying out any work on the power tool (e.g. maintenance, tool change etc.), remove the battery from the power tool. There is risk of injury from unintentionally pressing the on/off switch.

The machine head can be rotated in 90° increments. In this way, the on/off switch can be brought into a more favourable handling position for particular applications, e.g. for left-handed tool users.

Completely unscrew the 4 screws (➊). Rotate the machine head carefully, without removing it from the housing, into the new position (➋). Screw in and retighten the 4 screws (➌).