# Inserting/Removing the Fleece Filter Bag (see figures A−B)

You can use a fleece filter bag (20) for dry extraction. This makes the dust easier to dispose of.

Open the catches (13) and remove the top part of the dust extractor (12).

Swivel the fleece filter bag holder (19) upwards until it engages in a horizontal position.

Push the fleece filter bag (20) all the way into the fleece filter bag holder (19).

To remove it, push the fleece filter bag (20) downwards slightly and pull it out of the fleece filter bag holder (19).

To extract without a fleece filter bag, fold the fleece filter bag holder (19) back down: To do this, press the locks (21) of the fleece filter bag holder together, swivel the fleece filter bag holder down and press it against the wall of the container until it engages.

Put the top part of the dust extractor (12) back on and connect the container (3) with the top part of the dust extractor (12) by closing the catches (13).